**DERIVING A CONSTITUTIVE MODEL FOR PREDICTING THE RHEOLOGICAL RESPONSE OF DRUG-CARRYING PARTICLES**

**P. S. Stephanou1,\***

1 Thermodynamics and Transport Phenomena Laboratory (T2PL), Department of Chemical Engineering, Cyprus University of Technology, Corner of Athinon and Anexartisias, 57, 3036 Limassol, Cyprus

*\*pavlos.stefanou@cut.ac.cy*

**ABSTRACT**

In the past few decades, nanotechnology has been employed to provide breakthroughs in the diagnosis and treatment of several diseases using drug-carrying particles (DCPs). [1] In such an endeavor, the optimal design of DCPs is paramount, which necessitates the use of an accurate and trustworthy constitutive model in computational fluid dynamics (CFD) simulators. We herein introduce a continuum model to predict the rheological response of suspensions of DCPs in blood [2]. The model is developed using non-equilibrium thermodynamics [3] to guarantee thermodynamic admissibility. Red blood cells (RBCs) are modeled as deformed droplets with a constant volume that are able to aggregate; this is accomplished by using two structural variables: a constrained contravariant second-rank tensor, , such that is equal to the volume of an RBC, to characterize the deformation of RBCs, [4] and an additional structural variable, , to properly characterize the network formed by RBCs, leading to the exhibition of a yield stress [5]. Next, we consider particles as rigid spheroids whose orientation is characterized via an orientation tensor constrained to have a constant trace (due to particle rigidity). The model predictions are compared favorably against rheological data for both spherical and non-spherical particles immersed in non-aggregating blood [6]. Our model’s use in CFD simulations will allow the execution of in silico trials for the testing of DCPs in virtual patients.

**KEYWORDS:** Blood, Non-equilibrium thermodynamics, Particle, Viscosity, Normal stresses

**REFERENCES**

[1] Irvine D. J., & Dane E. L. (2020). *Nat Rev Immunol* 20:321–334.

[2] Stephanou, P. S. (2021). *Rheol. Acta* 60 (10): 603–616.

[3] Beris, A. N., & Edwards, B. J., (1994). Thermodynamics of Flowing Systems: with Internal Microstructure, Oxford University Press, New York.

[4] Stephanou, P. S. & Tsimouri, I. C. (2020). *Soft Matter* 16 (32):7585–7597.

[5] Stephanou, P. S. (2020). *Phys. Fluids* 32 (10): 103103

[6] Antonova, N., Koseva, N., Kowalczuk, A., Riha, P., & Ivanov, I., (2014). *Appl. Rheol.* 24: 35190.